Arduino shield v1.0 for Robco 01

Voltage: 18-24 V (DC)

Current: 3 A

by Alexey Shamraev 2019

off/on power usb